
How to upgrade:

1. HOLD 【MON】+【FUN】 key when power on radio, release the key when red light flashes;
2. connect PC cable and radio;
3. running the firmware “QXCodePro\_Update\_1.05.exe” as an administrator;
4. hit “open update file”, choose right comport “at779\_UV\_500\_v2\_29\_3\_VOX 2021\_4\_14.spi “ , speed set 115200. choose Duplex



1. Hit “Write”. Please reset radio after upgrade;

How to reset:

1. Hold “V/M” key when power on radio to enter band selection;
2. Press UP/DOWN key to choose full bands “136-174,400-470”, then power off radio;
3. Repeat the above steps, hold “V/M” key when power on radio to enter band selection; Press UP/DOWN key to choose GMRS bands, then power off radio;